LightNOW Premier Level Sponsor
2019 May 30, 2019
Impact Architectural Lighting

Fun, flirty, 2 sizes fit most. The new min!skrt from Impact features mid-power LED’s arrayed around a see-thru center.  Easy on the eyes, the diffusion acrylic has 72% light transmission with a matte surface providing light-scattering, glare-reduction and colorless diffusion that significantly reduces color shift of the LED’s.  Choose between a suspension using colorful cloth covered power cords and ultra-thin cables or go cordless with our POC, power-over-cable option.  The secondary inner diffuser is available in spun aluminum creating an optical play of light and dark spaces or choose the thermoformed acrylic diffuser for a dynamic boost to the lumen output.  A constant current, class P, programmable driver with 1% minimum dimming level allows for full control when you need to turn the lights down low.  Our palette of 15 standard colors with the option of any RAL color allows the min!skrt to complement any interior space.  Try one on today.

http://lightsearch.com/cgi-bin/counter.pl?idnum=1464