LightNOW Special Products Issue - Winter 2020

Company Name: FC Lighting

Product Title: FCSL2000 Series Step Lights

Product Description:

To ensure greater lifetime performance the SL2000 Series Step Lights were built and tested to IP68 standard. They use anti-wicking wiring cable to prevent water siphoning into the fixture, injection molded silicone seals for the optical/driver unit and a breather vent that allows air molecules in while keeping water out. They ship with waterproof wire nuts to complete proper wiring. The fastener-free faceplates have a clean, tamper-free look. They snap-in to the mounted Back Box, flush to the finished wall. Back Boxes are available for early shipment. The 13" x 4.5" faces have four aluminum and two stainless steel designs.

http://lightsearch.com/cgi-bin/counter.pl?idnum=1820

https://www.fclighting.com/media/newsletter/202005-FCSL2000/